Python version: 3.8.8 (Anaconda)

Complier: Spyder

Library & Dependency: No extra dependencies need to be downloaded. But make sure both “thorlabs\_DDS050.py” and “thorlabs\_DDS100.py” are in the same pathway as your main code

Extra: go to Device Manager, find Thorlabs 'APT USB device' (under USB controllers) and on the 'advanced' tab select the 'load VCP' check box to enable COM port